Asbestos Management Plan
ASBESTOS MANAGEMENT PLAN
Fillable template aligned with AHERA (40 CFR Part 763) and OSHA (29 CFR 1910.1001 / 1926.1101)
How to use this template: Replace the bracketed prompts and fill in the tables below to document your building's asbestos-containing materials (ACM), inspections, response actions, and ongoing operations and maintenance (O&M) program. Delete any sections that do not apply to your facility. This template is a starting point only — confirm the specific requirements that apply to your building, jurisdiction, and occupancy with a qualified asbestos professional and current federal, state, and local regulations before finalizing.
1. Facility & Plan Administration
Facility / building name:  	
Address:  	
Building owner / operator:  	
Designated person (AHERA) / program manager:  	
Contact email and phone:  	
Plan effective date:  	
Next scheduled review date:  	
2. Regulatory Applicability
Identify which frameworks apply to this building. Check all that apply:
1. AHERA — 40 CFR Part 763, Subpart E (public and non-profit private K-12 schools)
1. OSHA General Industry — 29 CFR 1910.1001 (general building O&M and worker exposure)
1. OSHA Construction — 29 CFR 1926.1101 (renovation, demolition, abatement work)
1. EPA NESHAP — 40 CFR Part 61, Subpart M (renovation and demolition notifications)
1. State / local asbestos program requirements: [enter applicable program(s)]
3. Asbestos-Containing Materials (ACM) Inventory
List each known or assumed ACM. Materials not sampled should be treated as ACM (“assumed”) until laboratory analysis proves otherwise.
	Location / Room
	Material / Use
	Type (surfacing, TSI, misc.)
	Friable? (Y/N)
	Est. Quantity
	Condition

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


4. Inspection & Assessment Records
Record the original inspection and each assessment of ACM condition.
	Date
	Inspector / Accreditation #
	Areas Inspected
	Assessment / Hazard Category
	Samples Collected

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


5. Response Actions & Abatement
Document the selected response action for each material (repair, encapsulation, enclosure, removal, or O&M).
	ACM / Location
	Response Action
	Reason
	Contractor
	Start Date
	Completion Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


6. Operations & Maintenance (O&M) Program
Describe the O&M program used to manage in-place ACM and minimize fiber release during routine activities:
1. Work practices and controls for activities that may disturb ACM
1. Permit / work-authorization process before drilling, cutting, or renovation
1. Cleaning procedures (HEPA vacuum, wet methods) and prohibited practices
1. Personal protective equipment (PPE) and respiratory protection requirements
1. Procedures for responding to fiber-release episodes and damaged ACM
O&M program administrator:  	
7. Periodic Surveillance (Every 6 Months)
AHERA requires visual surveillance of all known or assumed ACM at least once every 6 months.
	Surveillance Date
	Performed By
	Areas Reviewed
	Changes in Condition
	Action Taken

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


8. Reinspection (Every 3 Years)
AHERA requires a full reinspection by an accredited inspector at least once every 3 years.
	Reinspection Date
	Accredited Inspector / #
	Findings
	Plan Updates Required
	Next Due

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


9. Training & Awareness
Track awareness and accredited training for staff and maintenance / custodial workers.
	Name
	Role
	Training Type
	Date Completed
	Refresher Due

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


10. Notification & Communication
1. Annual written notification to building occupants, parents, and staff of plan availability and ACM activities (AHERA)
1. Notification to workers and contractors of ACM locations before work begins
1. NESHAP renovation/demolition notification to the appropriate regulatory agency, when applicable
Person responsible for notifications:  	
11. Recordkeeping
Maintain the following records and identify where each is stored:
1. Inspection, reinspection, and surveillance reports
1. Laboratory analysis results and sampling data
1. Response action and abatement documentation, including disposal manifests
1. Training records and accreditation certificates
1. Notifications issued and contractor work authorizations
Records location / system:  	
12. Plan Review & Approval
	Name
	Title
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	


Review and update this plan at least annually, and whenever ACM is added, disturbed, abated, or changes condition.
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